**Out of ramps unloading – tanks with liquid raw materials - standard of fully prepared vehicle for unloading**

**WRONG WAY:** The vehicle has no safety chock under its back wheel, orange and white cones with sign: „ Caution! Loading/Unloading in progress! “, are not placed in front of and behind the vehicle and valves are outside the area of leakage sump.

**RIGHT WAY:** Back wheel of the vehicle is blocked by safety chock, orange and white cones with sign: „Caution! Loading/Unloading in progress! “, are placed in front of and behind the vehicle, valves are above the area of leakage sump (see the pictures bellow)– **only vehicle that meets all these requirements can be unloaded.**

The leakage sump area is defined by drainage ditch.



Cone placed in front of the vehicle

**YES!!!**



Cone placed behind the vehicle

Valves placed above the leakage sump area

**YES!!!**



Back wheel blocked by safety chock

**YES!!!**