**Loading/ unloading on the ramp – standard of fully prepared vehicle for loading/ unloading**

**WRONG WAY:** **It is not allowed to load/ unload** the vehicle without safety chock under its back wheel.

**NO!!!**

**RIGHT WAY:** The back wheel of the vehicle **must always be blocked** by safety chock. Before leaving the loading/ unloading area, the driver checks whether the safety chock is removed from the back wheel and returned back to its place.

Back wheel blocked by safety chock

**YES!!!**

Place for safety chocks

Track loading area must be clean (no debris, oil spills etc.).



**YES!!!**

After hanging the keys from the vehicle on the keys rack, the driver stays in a designated area.