**Out of ramps (free place) loading/ unloading - standard of fully prepared vehicle for loading/ unloading**

**WRONG WAY:** **:** **It is not allowed to load/ unload** the vehicle without safety chock under its back wheel, without tarp taken down, without replaced elements ensuring the load and when orange and white cones with sign: „ Caution! Loading/Unloading in progress! “, are not placed in front of and behind the vehicle (see the picture bellow).



**NO!!!**

**RIGHT WAY:** Back wheel of the vehicle is blocked by safety chock, tarp is taken down, all elements securing the load and the other truck equipment are removed as well as the disorder (e. g. fragments of pallets etc.). Orange and white cones with sign: „Caution! Loading/Unloading in progress! “, must be placed in front of and behind the vehicle (see the picture bellow)– **only vehicle that meets all these requirements can be loaded/ unloaded.**

****

Cones placed in front of and behind the vehicle

Back wheel blocked by safety chock

Elements securing the load are removed

**YES!!!**